
  Series IX version 8.12.00             Version date: 18 Jul 2000

  Sample ID: PE02                       Test Date: 22 Jan 2013

  Test Type: Tensile                    Method: 3

  Operator Name: DING                   Edit date: -------

  Units: US Customary                   Geometry: Rectangular

  Number of specimens: 0                Number of channels: 2

  Machine type: 4200/4300/4400          Machine Control: STANDARD

  Data Rate: 6.667000 pts/sec           Extensometer: Disabled

  Crosshead Speed:    1.00000 in/min

  Second Speed: ------- 

  Temperature: 73 Deg F                 Humidity: 50 %

  Auto-start: Disabled                  Separate dimension entry: Enabled

  User Defined Fields:
      1:[                    ][                                        ]
      2:[                    ][                                        ]
      3:[                    ][                                        ]
      4:[                    ][                                        ]
      5:[                    ][                                        ]

  Auxiliary Sample Inputs:
      1: 0.000000 
      2: 0.000000 
      3: 0.000000 
      4: 0.000000 
      5: 0.000000 
      6: 0.000000 
      7: 0.000000 
      8: 0.000000 
      9: 0.000000 

  Sample comments:
    [                                                               ]
    [                                                               ]

   ___________________________________________________
